IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [VersionGUID: 6179efc5-99d9-4180-8e69-dbf50a19da6b, NumberOfSaves: 11]"
Description: "CoordinateReference [CoordinateBase: Internal Origin, ProjectSite: Internal]"
Description: "ExchangeRequirement [Architecture]"
Time stamp: "2025-09-10T12:27:26+01:00"
Preprocessor: "ODA SDAI 24.6"
Originating system: "Autodesk Revit 24.3.30.11 (ENU) - IFC 24.2.0.49"
Application: "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)"

People and organizations
  Person "marvinWLEQB" of Organization (no name given)
  Owner history of Person "marvinWLEQB" of Organization (no name given) | application "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)" | change NOCHANGE | created 1754048326 (2025-08-01T11:38:46Z)

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  AREADENSITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 45° 45′ 37.023925″ | longitude 21° 14′ 26.78009″ | elevation above sea level 0.
    IFCBUILDING | postal address: "45.7602844238281", "21.2407722473145"
      IFCBUILDINGSTOREY "B2__ABOVE Slab" | long name "B2__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation -612.00000000000011
      IFCBUILDINGSTOREY "B1__ABOVE Slab" | long name "B1__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation -312.00000000000023
      IFCBUILDINGSTOREY "L00__ABOVE Slab" | long name "L00__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation -12.000000000000195
        contains 1 element
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | object type "wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp:WS25" | COLUMN | names: "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | material: constituents ("_MASONRY__Timber Block__Triqbriq, X": "_MASONRY__Timber Block__Triqbriq, X", "_MASONRY__Timber Block__Triqbriq, Y": "_MASONRY__Timber Block__Triqbriq, Y")
      IFCBUILDINGSTOREY "L01__ABOVE Slab" | long name "L01__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation 272.99999999999983
      IFCBUILDINGSTOREY "L02__ABOVE Slab" | long name "L02__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation 557.99999999999977
      IFCBUILDINGSTOREY "L03__ABOVE Slab" | long name "L03__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation 842.99999999999989
      IFCBUILDINGSTOREY "L04__ABOVE Slab" | long name "L04__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation 1128.
      IFCBUILDINGSTOREY "L05__ABOVE Slab" | long name "L05__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation 1413.
      IFCBUILDINGSTOREY "L06__ABOVE Slab" | long name "L06__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation 1697.9999999999998
      IFCBUILDINGSTOREY "L07__ABOVE Slab" | long name "L07__ABOVE Slab" | object type "Level:ABOVE SLAB__Symbols Both Ends" | elevation 1983.

Types
  IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | COLUMN | 1 occurrence | material: constituents ("_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, X", "_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, Y")