IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [ContentGUID: d45b1106-0c7a-46e1-869b-c6a7bbcc7ea5, VersionGUID: 118b0530-1591-4ac2-8939-a10ffb714872, NumberOfSaves: 70]"
Description: "CoordinateReference [CoordinateBase: Internal Origin, ProjectSite: Internal]"
Description: "ExchangeRequirement [Architecture]"
File name: "3dv__Detail__15__211, WS25, Door, F90, Vertical_WIP Copy 1 Copy 1.ifc"
Time stamp: "2025-12-19T14:29:19+01:00"
Preprocessor: "ODA SDAI 25.12"
Originating system: "Autodesk - Revit 26.3.0.37 (ENU) - 26.4.1.0"
Application: "Autodesk Revit 2026 (ENU)" version "2026" identifier "Revit" by Organization "Autodesk Revit 2026 (ENU)"

People and organizations
  Person "marvinWLEQB" of Organization (no name given)
  Owner history of Person "marvinWLEQB" of Organization (no name given) | application "Autodesk Revit 2026 (ENU)" version "2026" identifier "Revit" by Organization "Autodesk Revit 2026 (ENU)" | change NOCHANGE | created 1765556194 (2025-12-12T16:16:34Z)

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 45° 45′ 37.023925″ | longitude 21° 14′ 26.78009″ | elevation above sea level 0.
    IFCBUILDING | postal address: "45.7602844238281", "21.2407722473145"
      IFCBUILDINGSTOREY "B2__ABOVE Slab" | long name "B2__ABOVE Slab" | elevation -612.00000000000011
      IFCBUILDINGSTOREY "B1__ABOVE Slab" | long name "B1__ABOVE Slab" | elevation -312.00000000000023
      IFCBUILDINGSTOREY "L00__ABOVE Slab" | long name "L00__ABOVE Slab" | elevation -12.000000000000195
        contains 33 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floors : Floor : flr__STRUCTURE__Wood Beams 15cm+insu__TriqBriq 2" | FLOOR | names: "Floors : Floor : flr__STRUCTURE__Wood Beams 15cm+insu__TriqBriq 2" | material: constituents "Floor:flr__STRUCTURE__Wood Beams 15cm+insu__TriqBriq 2" ("_STRUCTURE__Wood": "_STRUCTURE__Wood", "_FCD LAYERS__Insulation__Wood-fiber__Steico": "_FCD LAYERS__Insulation__Wood-fiber__Steico")
          1 x IFCBEAM | type IFCBEAMTYPE "Structural Framing : sfr__WOOD__Rectangular__sf : 15 x 1cm" | BEAM | names: "Structural Framing : sfr__WOOD__Rectangular__sf : 15 x 1cm" | material: "_STRUCTURE__Wood"
          1 x IFCSLAB | type IFCSLABTYPE "Floors : Floor : flr__INT COVERING__Parquet" | FLOOR | names: "Floors : Floor : flr__INT COVERING__Parquet" | material: constituents "Floor:flr__INT COVERING__Parquet" ("_FINISH STAIR__Int__Parquet Flooring__Stairs": "_FINISH STAIR__Int__Parquet Flooring__Stairs", "_FLR LAYERS__Screed, SL 0.5%__Semi-dry CEM, Rc ≥ 22.5 N/mm²": "_FLR LAYERS__Screed, SL 0.5%__Semi-dry CEM, Rc ≥ 22.5 N/mm²", "_FLR COVERING__Polished Concrete": "_FLR COVERING__Polished Concrete", "_FCD VENT LAYERS__Support Board__OSB 3": "_FCD VENT LAYERS__Support Board__OSB 3")
          2 x IFCWALL | type IFCWALLTYPE "Walls : Basic Wall : wll__EXT ENCLOSURE__Spritzkork, Wood Insulation 8.4cm__TriqBriq, FS.1" | names: "Walls : Basic Wall : wll__EXT ENCLOSURE__Spritzkork, Wood Insulation 8.4cm__TriqBriq, FS.1" | material: constituents "Basic Wall:wll__EXT ENCLOSURE__Spritzkork, Wood Insulation 8.4cm__TriqBriq, FS.1" ("_FCD FINISH__Mineral Render__Combed, H L/O__Capatect Kreativeffekt "Filigrano"__White": "_FCD FINISH__Mineral Render__Combed, H L/O__Capatect Kreativeffekt "Filigrano"__White", "_STRUCTURE__Wood Solid": "_STRUCTURE__Wood Solid", "_FCD LAYERS__Insulation__Wood-fiber__Steico": "_FCD LAYERS__Insulation__Wood-fiber__Steico")
          2 x IFCWALL | type IFCWALLTYPE "Walls : Basic Wall : wll__INT FINISH__Spritzkork, Lime - CEM Plaster 2.4cm TRIQBRIQ" | names: "Walls : Basic Wall : wll__INT FINISH__Spritzkork, Lime - CEM Plaster 2.4cm TRIQBRIQ" | material: constituents "Basic Wall:wll__INT FINISH__Spritzkork, Lime - CEM Plaster 2.4cm TRIQBRIQ" ("_WLL & CLG FINISHES__Lime - CEM Plaster": "_WLL & CLG FINISHES__Lime - CEM Plaster", "_FCD LAYERS__Insulation__EPS 120__Austrotherm EPS A120": "_FCD LAYERS__Insulation__EPS 120__Austrotherm EPS A120")
          1 x IFCBEAM | type IFCBEAMTYPE "Structural Framing : sfr__WOOD__Rectangular__sf : 15 x 25cm" | BEAM | names: "Structural Framing : sfr__WOOD__Rectangular__sf : 15 x 25cm" | material: "_MASONRY__Timber Block__Triqbriq, Filler"
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Ceilings : Compound Ceiling : clg__INT COVERING__Wood" | CEILING | names: "Ceilings : Compound Ceiling : clg__INT COVERING__Wood" | material: "_STRUCTURE__Wood Solid"
          1 x IFCWALL | type IFCWALLTYPE "Walls : Basic Wall : wll__UNCLASSIFIED__Randdämmstreifen 1.5cm" | names: "Walls : Basic Wall : wll__UNCLASSIFIED__Randdämmstreifen 1.5cm" | material: constituents "Basic Wall:wll__UNCLASSIFIED__Randdämmstreifen 1.5cm" ("_FCD LAYERS__Insulation__EPS 120__Austrotherm EPS A120": "_FCD LAYERS__Insulation__EPS 120__Austrotherm EPS A120")
          1 x IFCWINDOW | type IFCWINDOWTYPE "Windows : wdw_s__PANEL__Mobile, Hung, Interior__wp : Glazed, Bottom&side hung" | WINDOW | names: "Windows : wdw_s__PANEL__Mobile, Hung, Interior__wp : Glazed, Bottom&side hung" | material: constituents ("Miscellaneous_Profile_Aluminium": "Miscellaneous_Profile_Aluminium", "Unassigned_Glazing": "Unassigned_Glazing")
          1 x IFCWINDOW | type IFCWINDOWTYPE "Windows : wdw_s__PROFILE__Frame__wp : Wood" | WINDOW | names: "Windows : wdw_s__PROFILE__Frame__wp : Wood" | material: "_WINDOW__Profile__Aluminium"
          1 x IFCWINDOW | type IFCWINDOWTYPE "Windows : wdw_s__PROFILE__Frame__wp : Wood" | WINDOW | names: "Windows : wdw_s__PROFILE__Frame__wp : Wood" | material: "_WINDOW__Profile__Aluminium"
          1 x IFCWINDOW | type IFCWINDOWTYPE "Windows : wdw_s__PROFILE__Frame__wp : Wood" | WINDOW | names: "Windows : wdw_s__PROFILE__Frame__wp : Wood" | material: "_WINDOW__Profile__Aluminium"
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Ceilings : Compound Ceiling : clg__INT COVERING__, GB 1.5cm__12.5(A) 3" | CEILING | names: "Ceilings : Compound Ceiling : clg__INT COVERING__, GB 1.5cm__12.5(A) 3" | material: "_WLL & CLG FINISHES__Lime - CEM Plaster"
          1 x IFCBEAM | type IFCBEAMTYPE "Structural Framing : Light Gauge-Angles : L150 x 150" | BEAM | names: "Structural Framing : Light Gauge-Angles : L150 x 150" | material: "Metal - Light Gauge"
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Columns : wll__TIMBER CORE__Triqbriq__lb : WS25" | COLUMN | names: "Columns : wll__TIMBER CORE__Triqbriq__lb : WS25" | material: "<Unnamed>"
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | COLUMN | names: "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | material: constituents ("_MASONRY__Timber Block__Triqbriq, X": "_MASONRY__Timber Block__Triqbriq, X", "_MASONRY__Timber Block__Triqbriq, Y": "_MASONRY__Timber Block__Triqbriq, Y")
          1 x IFCWALL | type IFCWALLTYPE "Columns : wll_s__DECOUPLING BEAM__Rectangular__wp : Wood" | SOLIDWALL | names: "Columns : wll_s__DECOUPLING BEAM__Rectangular__wp : Wood" | material: "_STRUCTURE__Wood Solid"
          6 x IFCWALL | type IFCWALLTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp1 : WS25 2" | SOLIDWALL | names: "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp1 : WS25 2" | material: "Miscellaneous__Timber Block__Triqbriq, Y"
          1 x IFCWALL | type IFCWALLTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp1 : WS25 2" | SOLIDWALL | names: "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp1 : WS25 2" | material: "Miscellaneous__Timber Block__Triqbriq, Y"
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp : WS25" | COLUMN | names: "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp : WS25" | material: constituents ("_MASONRY__Timber Block__Triqbriq, X": "_MASONRY__Timber Block__Triqbriq, X", "_MASONRY__Timber Block__Triqbriq, Y": "_MASONRY__Timber Block__Triqbriq, Y")
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models : Generic Models 5 : Generic Models 5" | names: "Generic Models : Generic Models 5 : Generic Models 5" | material: "<Unnamed>"
      IFCBUILDINGSTOREY "L01__ABOVE Slab" | long name "L01__ABOVE Slab" | elevation 272.99999999999983
      IFCBUILDINGSTOREY "L02__ABOVE Slab" | long name "L02__ABOVE Slab" | elevation 557.99999999999977
      IFCBUILDINGSTOREY "L03__ABOVE Slab" | long name "L03__ABOVE Slab" | elevation 842.99999999999989
      IFCBUILDINGSTOREY "L04__ABOVE Slab" | long name "L04__ABOVE Slab" | elevation 1128.
      IFCBUILDINGSTOREY "L05__ABOVE Slab" | long name "L05__ABOVE Slab" | elevation 1413.
      IFCBUILDINGSTOREY "L06__ABOVE Slab" | long name "L06__ABOVE Slab" | elevation 1697.9999999999998
      IFCBUILDINGSTOREY "L07__ABOVE Slab" | long name "L07__ABOVE Slab" | elevation 1983.

Types
  IFCSLABTYPE "Floors : Floor : flr__STRUCTURE__Wood Beams 15cm+insu__TriqBriq 2" | FLOOR | 1 occurrence | material: constituents "Floor:flr__STRUCTURE__Wood Beams 15cm+insu__TriqBriq 2" ("_STRUCTURE__Wood": "_STRUCTURE__Wood", "_FCD LAYERS__Insulation__Wood-fiber__Steico": "_FCD LAYERS__Insulation__Wood-fiber__Steico")
  IFCBEAMTYPE "Structural Framing : sfr__WOOD__Rectangular__sf : 15 x 1cm" | BEAM | 1 occurrence | material: "_STRUCTURE__Wood"
  IFCSLABTYPE "Floors : Floor : flr__INT COVERING__Parquet" | FLOOR | 1 occurrence | material: constituents "Floor:flr__INT COVERING__Parquet" ("_FINISH STAIR__Int__Parquet Flooring__Stairs": "_FINISH STAIR__Int__Parquet Flooring__Stairs", "_FLR LAYERS__Screed, SL 0.5%__Semi-dry CEM, Rc ≥ 22.5 N/mm²": "_FLR LAYERS__Screed, SL 0.5%__Semi-dry CEM, Rc ≥ 22.5 N/mm²", "_FLR COVERING__Polished Concrete": "_FLR COVERING__Polished Concrete", "_FCD VENT LAYERS__Support Board__OSB 3": "_FCD VENT LAYERS__Support Board__OSB 3")
  IFCWALLTYPE "Walls : Basic Wall : wll__EXT ENCLOSURE__Spritzkork, Wood Insulation 8.4cm__TriqBriq, FS.1" | STANDARD | 2 occurrences | material: constituents "Basic Wall:wll__EXT ENCLOSURE__Spritzkork, Wood Insulation 8.4cm__TriqBriq, FS.1" ("_FCD FINISH__Mineral Render__Combed, H L/O__Capatect Kreativeffekt "Filigrano"__White": "_FCD FINISH__Mineral Render__Combed, H L/O__Capatect Kreativeffekt "Filigrano"__White", "_STRUCTURE__Wood Solid": "_STRUCTURE__Wood Solid", "_FCD LAYERS__Insulation__Wood-fiber__Steico": "_FCD LAYERS__Insulation__Wood-fiber__Steico")
  IFCWALLTYPE "Walls : Basic Wall : wll__INT FINISH__Spritzkork, Lime - CEM Plaster 2.4cm TRIQBRIQ" | STANDARD | 2 occurrences | material: constituents "Basic Wall:wll__INT FINISH__Spritzkork, Lime - CEM Plaster 2.4cm TRIQBRIQ" ("_WLL & CLG FINISHES__Lime - CEM Plaster": "_WLL & CLG FINISHES__Lime - CEM Plaster", "_FCD LAYERS__Insulation__EPS 120__Austrotherm EPS A120": "_FCD LAYERS__Insulation__EPS 120__Austrotherm EPS A120")
  IFCBEAMTYPE "Structural Framing : sfr__WOOD__Rectangular__sf : 15 x 25cm" | BEAM | 1 occurrence | material: "_MASONRY__Timber Block__Triqbriq, Filler"
  IFCCOVERINGTYPE "Ceilings : Compound Ceiling : clg__INT COVERING__Wood" | CEILING | 3 occurrences
  IFCWALLTYPE "Walls : Basic Wall : wll__UNCLASSIFIED__Randdämmstreifen 1.5cm" | STANDARD | 1 occurrence | material: constituents "Basic Wall:wll__UNCLASSIFIED__Randdämmstreifen 1.5cm" ("_FCD LAYERS__Insulation__EPS 120__Austrotherm EPS A120": "_FCD LAYERS__Insulation__EPS 120__Austrotherm EPS A120")
  IFCWINDOWTYPE "Windows : wdw_s__PANEL__Mobile, Hung, Interior__wp : Glazed, Bottom&side hung" | WINDOW | 1 occurrence | material: constituents ("_SASH": "Miscellaneous_Profile_Aluminium", "_GLAZING": "Unassigned_Glazing") | property sets: Windows : wdw_s__PANEL__Mobile, Hung, Interior__wp : Glazed, Bottom&side hung
  IFCWINDOWTYPE "Windows : wdw_s__PROFILE__Frame__wp : Wood" | WINDOW | 1 occurrence | material: "_WINDOW__Profile__Aluminium" | property sets: Windows : wdw_s__PROFILE__Frame__wp : Wood
  IFCWINDOWTYPE "Windows : wdw_s__PROFILE__Frame__wp : Wood" | WINDOW | 1 occurrence | material: "_WINDOW__Profile__Aluminium" | property sets: Windows : wdw_s__PROFILE__Frame__wp : Wood
  IFCWINDOWTYPE "Windows : wdw_s__PROFILE__Frame__wp : Wood" | WINDOW | 1 occurrence | material: "_WINDOW__Profile__Aluminium" | property sets: Windows : wdw_s__PROFILE__Frame__wp : Wood
  IFCCOVERINGTYPE "Ceilings : Compound Ceiling : clg__INT COVERING__, GB 1.5cm__12.5(A) 3" | CEILING | 2 occurrences
  IFCBEAMTYPE "Structural Framing : Light Gauge-Angles : L150 x 150" | BEAM | 1 occurrence | material: "Metal - Light Gauge"
  IFCCOLUMNTYPE "Columns : wll__TIMBER CORE__Triqbriq__lb : WS25" | COLUMN | 1 occurrence | material: "<Unnamed>"
  IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | COLUMN | 3 occurrences | material: constituents ("_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, X", "_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, Y")
  IFCWALLTYPE "Columns : wll_s__DECOUPLING BEAM__Rectangular__wp : Wood" | SOLIDWALL | 1 occurrence | material: "_STRUCTURE__Wood Solid"
  IFCWALLTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp1 : WS25 2" | SOLIDWALL | 6 occurrences | material: "Miscellaneous__Timber Block__Triqbriq, Y"
  IFCWALLTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp1 : WS25 2" | SOLIDWALL | 1 occurrence | material: "Miscellaneous__Timber Block__Triqbriq, Y"
  IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp : WS25" | COLUMN | 1 occurrence | material: constituents ("_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, X", "_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, Y")
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models : Generic Models 5 : Generic Models 5" | 1 occurrence | material: "<Unnamed>"

Property sets
  Windows : wdw_s__PANEL__Mobile, Hung, Interior__wp : Glazed, Bottom&side hung | predefined | on 1 type object
  Windows : wdw_s__PROFILE__Frame__wp : Wood | predefined | on 3 type objects