IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [ContentGUID: d45b1106-0c7a-46e1-869b-c6a7bbcc7ea5, VersionGUID: 118b0530-1591-4ac2-8939-a10ffb714872, NumberOfSaves: 70]"
Description: "CoordinateReference [CoordinateBase: Internal Origin, ProjectSite: Internal]"
Description: "ExchangeRequirement [Architecture]"
File name: "3dv__Detail__15__101+113, WS25 Wall,EFH40.ifc"
Time stamp: "2025-12-19T14:27:32+01:00"
Preprocessor: "ODA SDAI 25.12"
Originating system: "Autodesk - Revit 26.3.0.37 (ENU) - 26.4.1.0"
Application: "Autodesk Revit 2026 (ENU)" version "2026" identifier "Revit" by Organization "Autodesk Revit 2026 (ENU)"

People and organizations
  Person "marvinWLEQB" of Organization (no name given)
  Owner history of Person "marvinWLEQB" of Organization (no name given) | application "Autodesk Revit 2026 (ENU)" version "2026" identifier "Revit" by Organization "Autodesk Revit 2026 (ENU)" | change NOCHANGE | created 1765556194 (2025-12-12T16:16:34Z)

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 45° 45′ 37.023925″ | longitude 21° 14′ 26.78009″ | elevation above sea level 0.
    IFCBUILDING | postal address: "45.7602844238281", "21.2407722473145"
      IFCBUILDINGSTOREY "B2__ABOVE Slab" | long name "B2__ABOVE Slab" | elevation -612.00000000000011
      IFCBUILDINGSTOREY "B1__ABOVE Slab" | long name "B1__ABOVE Slab" | elevation -312.00000000000023
      IFCBUILDINGSTOREY "L00__ABOVE Slab" | long name "L00__ABOVE Slab" | elevation -12.000000000000195
        contains 16 elements
          3 x IFCWALL | type IFCWALLTYPE "Walls : Basic Wall : wll__WP & INSULATION_1cm" | names: "Walls : Basic Wall : wll__WP & INSULATION_1cm" | material: constituents "Basic Wall:wll__WP & INSULATION_1cm" ("_FND LAYERS__Insulation__Foam Glass__Glapor": "_FND LAYERS__Insulation__Foam Glass__Glapor")
          1 x IFCWALL | type IFCWALLTYPE "Walls : Basic Wall : wll__INT FINISH__Spritzkork 0.4cm__TriqBriq, TN.1" | names: "Walls : Basic Wall : wll__INT FINISH__Spritzkork 0.4cm__TriqBriq, TN.1" | material: constituents "Basic Wall:wll__INT FINISH__Spritzkork 0.4cm__TriqBriq, TN.1" ("_WLL & CLG FINISHES__Spray-cork": "_WLL & CLG FINISHES__Spray-cork")
          1 x IFCWALL | type IFCWALLTYPE "Walls : Basic Wall : wll__WP & INSULATION__Foam Glass 20cm__On Heated Bsmt Wall, TriqBriq, IZ.1 4" | names: "Walls : Basic Wall : wll__WP & INSULATION__Foam Glass 20cm__On Heated Bsmt Wall, TriqBriq, IZ.1 4" | material: constituents "Basic Wall:wll__WP & INSULATION__Foam Glass 20cm__On Heated Bsmt Wall, TriqBriq, IZ.1 4" ("_FND LAYERS__Protection & Drainage Membrane__Dimple Sheet": "_FND LAYERS__Protection & Drainage Membrane__Dimple Sheet", "_FCD LAYERS__Adhesive__Cell Filling__Glapor": "_FCD LAYERS__Adhesive__Cell Filling__Glapor", "_FND LAYERS__Insulation__Foam Glass__Glapor": "_FND LAYERS__Insulation__Foam Glass__Glapor", "_FCD LAYERS__Adhesive__For Foam Glass__Glapor": "_FCD LAYERS__Adhesive__For Foam Glass__Glapor")
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Columns : wll__TIMBER CORE__Triqbriq__lb : WS25" | COLUMN | names: "Columns : wll__TIMBER CORE__Triqbriq__lb : WS25" | material: "<Unnamed>"
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp : WS25" | COLUMN | names: "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp : WS25" | material: constituents ("_MASONRY__Timber Block__Triqbriq, X": "_MASONRY__Timber Block__Triqbriq, X", "_MASONRY__Timber Block__Triqbriq, Y": "_MASONRY__Timber Block__Triqbriq, Y")
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | COLUMN | names: "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | material: constituents ("_MASONRY__Timber Block__Triqbriq, X": "_MASONRY__Timber Block__Triqbriq, X", "_MASONRY__Timber Block__Triqbriq, Y": "_MASONRY__Timber Block__Triqbriq, Y")
      IFCBUILDINGSTOREY "L01__ABOVE Slab" | long name "L01__ABOVE Slab" | elevation 272.99999999999983
      IFCBUILDINGSTOREY "L02__ABOVE Slab" | long name "L02__ABOVE Slab" | elevation 557.99999999999977
      IFCBUILDINGSTOREY "L03__ABOVE Slab" | long name "L03__ABOVE Slab" | elevation 842.99999999999989
      IFCBUILDINGSTOREY "L04__ABOVE Slab" | long name "L04__ABOVE Slab" | elevation 1128.
      IFCBUILDINGSTOREY "L05__ABOVE Slab" | long name "L05__ABOVE Slab" | elevation 1413.
      IFCBUILDINGSTOREY "L06__ABOVE Slab" | long name "L06__ABOVE Slab" | elevation 1697.9999999999998
      IFCBUILDINGSTOREY "L07__ABOVE Slab" | long name "L07__ABOVE Slab" | elevation 1983.

Types
  IFCWALLTYPE "Walls : Basic Wall : wll__WP & INSULATION_1cm" | STANDARD | 3 occurrences | material: constituents "Basic Wall:wll__WP & INSULATION_1cm" ("_FND LAYERS__Insulation__Foam Glass__Glapor": "_FND LAYERS__Insulation__Foam Glass__Glapor")
  IFCWALLTYPE "Walls : Basic Wall : wll__INT FINISH__Spritzkork 0.4cm__TriqBriq, TN.1" | STANDARD | 1 occurrence | material: constituents "Basic Wall:wll__INT FINISH__Spritzkork 0.4cm__TriqBriq, TN.1" ("_WLL & CLG FINISHES__Spray-cork": "_WLL & CLG FINISHES__Spray-cork")
  IFCWALLTYPE "Walls : Basic Wall : wll__WP & INSULATION__Foam Glass 20cm__On Heated Bsmt Wall, TriqBriq, IZ.1 4" | STANDARD | 1 occurrence | material: constituents "Basic Wall:wll__WP & INSULATION__Foam Glass 20cm__On Heated Bsmt Wall, TriqBriq, IZ.1 4" ("_FND LAYERS__Protection & Drainage Membrane__Dimple Sheet": "_FND LAYERS__Protection & Drainage Membrane__Dimple Sheet", "_FCD LAYERS__Adhesive__Cell Filling__Glapor": "_FCD LAYERS__Adhesive__Cell Filling__Glapor", "_FND LAYERS__Insulation__Foam Glass__Glapor": "_FND LAYERS__Insulation__Foam Glass__Glapor", "_FCD LAYERS__Adhesive__For Foam Glass__Glapor": "_FCD LAYERS__Adhesive__For Foam Glass__Glapor")
  IFCCOLUMNTYPE "Columns : wll__TIMBER CORE__Triqbriq__lb : WS25" | COLUMN | 1 occurrence | material: "<Unnamed>"
  IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Half Width__wp : WS25" | COLUMN | 4 occurrences | material: constituents ("_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, X", "_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, Y")
  IFCCOLUMNTYPE "Columns : wll_s__TIMBER BLOCK__Triqbriq, Full Width__wp : WS25" | COLUMN | 6 occurrences | material: constituents ("_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, X", "_TRIQBRIQ__Brick Subelement": "_MASONRY__Timber Block__Triqbriq, Y")